产品简介

**1000流明双尾按“量子系列”手电**

**量子纠缠，一种神奇而美丽的现象，让无数天才人物为之倾倒！SUNWAYMAN从中汲取灵感，推出轻触式不锈钢双尾按手电——Q系列产品！SUNWAYMAN G25C，业界双尾按手电升华之作，将传统双尾按手电的功能和操控进一步提高！不锈钢双尾按，轻触式按钮，主按钮控制电源，副按钮负责调光，分工明确，操控简单，容易上手，容易玩儿。手电关闭时可用副键一键快速调出爆闪，做到适时警戒和防范！精选CREE XM-L2 U2照明核心，亮度最高可达1000流明。筒身精密化设计和加工，可能是体积最小的18650电池手电，便于握取和携带。小巧、精致、便携的“双子座”G25C，是您工作、生活、出游的超强照明小助理！**

**1000 Lumens Dual-button Super-compact Powerful Flashlight**

**Inspired by the beautiful and mysterious quantum entanglement phenomenon, Sunwayman developed another new series of the stainless steel tail cap soft-contact dual-button switch- Q Series.SUNWAYMAN G25C is the upgraded dual-button switch model with improved performance and easy-operation. Stainless steel soft-contact dual-button at the tail, main button controls on/off and the other one to select desired output mode, very intuitive user interface. The Strobe mode can be activated directly even with the light turned off for emergencies. Fitted with CREE XM-L2 U2 LED, max output reaches 1000 lumens. Elaborately-designed and precisely-machined light body, this is one surprisingly-compact 18650 model, easy to grip and carry daily. The upgraded G25C is your ideal lighting tool for all of your adventures!**

**1000流明双尾按“双子座”手电**

SUNWAYMAN G25C，业界双尾按手电升华之作，将传统双尾按手电的功能和操控进一步提高！不锈钢双尾按，轻触式按钮，主按钮控制电源，副按钮负责调光，分工明确，操控简单，容易上手，容易玩儿。全新研发的手电功能模块，可快捷的转换为三种照明模式，分别为日用模式、户外模式、战术模式，让您在不同的使用环境下，能得到不同的照明模式，更加贴心和方便，做到适时警戒、搜索和防范！精选CREE XM-L2 U2照明核心，亮度最高可达1000流明。筒身精密化设计和加工，可能是体积最小的18650电池手电，便于握取和携带。小巧、精致、便携的“双子座”G25C，是您工作、生活、出游的超强照明小助理！

**1000 Lumens Dual-button Super-compact Powerful Flashlight**

SUNWAYMAN G25C is the upgraded dual-button switch model with improved performance and easy-operation. Stainless steel soft-contact dual-button at the tail, main button controls on/off and the other one to select desired output mode, very intuitive user interface. Thanks to the new circuit module developed, there are 3 types of mode-switching can be selected by users according to own preference. They are Daily, Outdoor and Tactical mode-switching. The Strobe mode can be activated directly even with the light turned off for emergencies. Fitted with CREE XM-L2 U2 LED, max output reaches 1000 lumens. Elaborately-designed and precisely-machined light body, this is one surprisingly-compact 18650 model, easy to grip and carry daily. The upgraded G25C is your ideal lighting tool for all of your adventures!

性能特点

●采用一颗Cree XM-L2 U2 LED，寿命均长达50,000小时；

●两个尾部按键，一个开关、一个调光，三种照明模式：

亮度和续航如下： 高亮档（1000流明，续航2小时）；中亮档（150流明，续航6小时），低亮档（16流明，续航80小时 ）；爆闪

●恒流电路，亮度恒定

●有效射程达208米

●使用一节18650电池电池或者两节CR123A电池；

●工作电压：2.8~6V

●采用优质金属光面反光杯，兼顾聚光和泛光，光斑完美

●体积：113mm (长) x30mm(头部直径)x25mm（尾部直径）

●重量：93.4g（不含电池）

●采用航天级铝合金制造，头部不锈钢压环；

●军规三级硬质氧化

●IPX-8级防水

●增韧超清晰钢化玻璃镜片，防刮耐磨

●附件：防水O圈、手绳、抱夹

Features

● CREE XM-L2 U2 LED, with a lifetime of up to 50,000 hours;

● Tail cap dual-push-button switches, one to control on/off, the other for selecting desired output mode, three types mode-switching;

Output & Runtime

High- 1000 Lumens, 2 hr.

Mid- 150 Lumens, 6 hrs.

Low- 16 Lumens, 80 hrs.

Strobe

● Constant current circuit, constant output

● Effective range of 208 meters

● Uses one single 18650 or two CR123A batteries

● Working voltage: 2.8~6V

● High quality metal smooth reflector maintains great throw distance and spread with an ideal beam pattern

● Dimensions: 113mm (length) x 30mm (head diameter) x 25mm (tail diameter)

● Weight: 93.4g（battery excluded）

● Aerospace-grade aluminum alloy, Stainless Steel retaining ring on the top

● Military Specification Type III- hard anodized body

● Waterproof, in accordance with IPX-8 standard

● Ultra-clear tempered glass lens resists scratches and impacts

● Accessories: Clip, Lanyard ,O-rings

操作方法

G25C手电有三种模式供用户选择：战术模式、执法模式、日用模式。

具体操作为同时按按下尾部POERW键（大按键）和我MODE键（小按键）快速拧松筒身再按紧，当拧紧筒身后电筒快速闪烁一次为战术模式，快闪二次为执法模式，快闪三次为日用模式。

1. 战术模式：灯灭时，轻按MODE键可瞬间点亮爆闪模式，松开后熄灭。轻按一次POWER键可打开手电，此时为高亮，再轻 按一次关闭手电，灯亮时轻按MODE键可在高亮与爆闪档之间切换，松手可停留在该档位，关闭亮度后不记忆档位， 下次开启亮度时仍为高亮。

2. 执法模式：手电未点亮时，轻按MODE键为爆闪，松手即灭，轻按一次POWER键可打开高亮，再按关闭亮度，灯亮时轻按 MODE键可在高低亮间切换，长按MODE键进入爆闪档，松手保留爆闪档，如此时轻按一次则回到爆闪前的档位，此模式下不记忆档位，当灯熄灭后下次按POWER键时则进入高亮档。

3. 日用模式：灯不亮时，轻按MODE键瞬间爆闪，松手即灭。轻按POWER键一下可打开手电亮度，再按关闭亮度。灯亮的情 况下轻按MODE键可在低、中、高亮间切换，长按可进入爆闪档，松手保留该档位，日用模式下所有档位匀有记忆， 况下轻按MODE键可在低、中、高亮间切换，长按可进入爆闪档，松手保留该档位，日用模式下所有档位匀有记忆，即下次开启时为关机前的档位。

Operation

G25C has three types of mode-switching: Daily, Outdoor and Tactical.

Depress and hold both the Power and Mode buttons at the tail cap, and at the same time swiftly loosen and tighten the light body, with the light flash once to enter Tactical mode-switching; twice to enter Outdoor and three times to activate Daily mode-switching.

1. Tactical Mode-switching: with the light turned off, slightly-depress the Mode button to activate Strobe and release to turn it off. Slightly-depress the Power button to turn on the light and it comes at High mode, another slight-depress will turn off the light. With the light turned on, slightly-depress the mode button to choose from High and Strobe, release to choose either mode. The light always comes at High mode when turning on.
2. Outdoor Mode-switching: with the light turned off, slightly-depress the Mode button to activate Strobe, release to turn it off. Slightly-depress the Power button to turn on the light at High, another depress to turn it off. When the light is turned on, slightly-depress the Mode button to choose from High and Low, depress-and-hold the Mode button to enter Strobe, if slightly-depress the Mode button again, the light will resume the mode used before turning on the Strobe. The light always comes at High mode when turning on.
3. Daily Mode-switching: with the light turned off, slightly-depress the Mode button to actiate Strobe and release to turn it off. Slightly-depress the Power button to turn on the light and another depress to turn it off. With the light turned on, slightly-depress the Mode button to choose from Low, Mid, High outputs. Depress-and-hold the Mode button to activate Strobe. This light has memory function under Daily system, it always come at the most recent mode used before turned off.

常见问题

1、 手电不能正常点亮，如何处理？

如果手电不能正常点亮或者发生闪烁的状况，请检查是否电池电量耗尽，并更换新的电池；如果更换了新电池依然不能正常点亮，请检查手电的电池正负极触点、导电切面是否有污物，并用干劲的清洁布清理，清理之后如果依然不能正常点亮，请联系您的手电销售商，按正常的保修流程进行保修；

2、 如何成为SUNWAYMAN的经销商

如果您对经销SUNWAYMAN产品感兴趣，请将您的基本信息以邮件的形式发往邮箱：info@sunwayman.com，SUNWAYMAN公司将在第一时间与您取得联系，商讨后继事宜。

另外您也可以推荐您认为有实力的本地经销商给SUNWAYMAN公司，如果您推荐的销售商最终与SUNWAYMAN公司达成合作，SUNWAYMAN公司将免费为您提供丰厚的礼品。

3、 如何获得SUNWAYMAN的最新产品信息或者各类活动信息？

您可经常登录www.sunwayman.com网站的新品频道或者新闻频道获取新品信息和各类活动信息；如果您愿意，您也可以用您的常用邮箱发邮件给：[info@sunwayman.com进行相关查询。](mailto:info@sunwayman.com进行相关查询。)

FAQs

1. I could not turn on the light normally, what’s my first step?

LED flashlight are solid state devices so any functional issues are typically 1 of 4 things; old batteries, bad contact, a failed switch or a failed component in the LED module.

Step #1: We know it seems obvious but the first thing you must do is insert fresh batteries. If that did not work please proceed to Step #2.

Step #2: Please check that the battery contacts are clean; this means the points where the +/- of the battery contact and also where the tail cap contacts the battery tube as the current from the negative electrode is transmitted via the lights switch, through the body of the light and up to the LED. Rubbing alcohol and/or a pencil eraser work well. The idea is to remove any grease outside of that on the threads of the light and switch bodies (please clean any grease off of the bottom edge of the battery tube). If that did not work please proceed to Step #3.

Step #3: It's time to take the switch out of the loop. Remove the switch or tail cap. Get something conductive and flexible - a paperclip, a small length of wire, etc. and 'jumper' from the bottom of the battery to the bottom of the battery edge tube where it is bare metal. This makes a circuit and will let us know if the problem is in the switch. If the light now goes on the odds are that the switch is the problem. Regardless of outcome please proceed to Step #4.

Step #4: Please contact the dealer where you purchased the light or your regional distributor for warranty service.

2. How does my company become a SUNWAYMAN dealer?

If you are interested in dealing with SUNWAYMAN, please contact us by sending email to info@sunwayman.com and we will get in touch with you immediately and proceed with a more detailed discussion.

Can you recommend a dealer? If you can recommend a local dealer to SUNWAYMAN and we end up establishing cooperation with the dealer you recommended, we will send you a great thank you gift!

3. How can I get latest information of SUNWAYMAN products or various activities?

Please visit our website www.sunwayman.com for the latest in product news and updates; you can also send email to info@sunwayman.com to inquire.

使用注意事项

※电池使用

1、电池类型：本手电使用一节18650电池或者两节CR123A节电池，使用充电电池时，请选用优质的带保护电路的充电电池；

2、电池更换：虽然本手电具有电池防反接设计，即使电池无意中装反，也不会损害手电电路和电池，但是为了提高您的手电使用效率，更换电池时希望您能一次性对准电池正负极；

3、手电长期不使用时，请将电池取出，以免发生电池漏液，损坏手电元器件。

※防水圈使用

1、手电出厂时防水圈会涂抹适量的润滑油，即可保证润滑延长防水圈的使用寿命，也更利于防水。当您发现您的手电防水圈处润滑油较少或已经没有，旋转螺纹，有滞涩感时，请及时在防水圈处涂抹一些润滑油；

2、手电长期使用以后会发生防水圈磨损，请及时更换包装内附送的防水圈。

CAUTION

Use of Battery

1. Battery: Uses one 18650 or two CR123A batteries;

2. Battery Replacement: to ensure performance of the flashlight and for your own safety, please be sure to select good quality same brand same capacity battery and make sure to insert battery correctly.

3. Please take out battery if you will not be using your light for an extended period to avoid battery leakage which may damage the flashlight components and parts.

Use of O-rings

1. The right amount of lubricant will be applied on the flashlight o-rings before shipping out in order to ensure smooth operation, extend the lifetime of the o-rings, and to increase water-resistance. When there is little or no lubricant on the o-rings and it's difficult to twist between threads, please apply lubricant on the o-rings in time.

2. The o-rings can be worn out due to long time use, please replace with spare o-rings attached in the package.

警告

1、此手电点亮后会发出高亮强光，请不要将光线照射自己或他人的眼睛，以免发生损害；

2、 请不要将此手电给小孩作为玩具玩耍，以免发生损害；

3、 支持环保，废旧的电池请不要随意丢弃，请交给指定的回收 点。

WARNING

1. SUNWAYMAN Flashlight are not toys but high output device, please do NOT shine the light directly in ANYONES eyes!

2. Please do not leave children unattended around our lights.

3. Please recycle! Please dispose of used batteries properly; do not throw them away or incinerate them.

网络保修卡注册

您可登录www.sunwayman.com客户服务频道，将您的手电编码注册，注册成功后，您将免费获得延长6个月的免费保修期，您手电的免费保修期最长可达30个月。

Internet Warranty Card Registration

Please visit www.sunwayman.com and go to the Customer Service link on our website to register the unique serial number on your flashlight. Successful registration will also entitle the registrant to a bonus 6 month extension of their Full Warranty bringing the available Full Warranty Period to 30 months.

售后条款

1、15日保修保换

  SUNWAYMAN手电自售出之日起15日内，在正常使用情况下，出现产品品质问题， 您可选择修理或者更换同型号同规格的新品；如同型号同规格的产品停止生产时或因其它原因不能在合理的时间内安排更换给您，则调换不低于原产品性能的同品牌产品；

2、24个月免费保修

  SUNWAYMAN手电自售出之日起24个月内，您在正常使用情况下，出现产品品质问题，则享受免费维修服务；

3、终身有限维护

   SUNWAYMAN公司将为您提供终身有限维护服务，即在您的手电超过24个月免费保修期后，出现手电故障，SUNWAYMAN可为您提供终身有偿维护和保修，费用以实际更换材料费用为准，不另收取人工费用；

4、网上注册，延长保修期

    SUNWAYMAN公司建议您到WWW.SUNWAYMAN.COM网站客户服务频道注册每支手电独一无二的产品编码，注册成功后您将免费获得6个月的免费保修期，即您的手电的免费保修期最长可达30个月；

5、请您直接联系购买时的经销商

    您保修时凭SUNWAYMAN《保修卡》、购物发票或收据或网上购物时经销商提供的销售凭证与经销商联系，由经销商为您提供售后服务，SUNWAYMAN对经销商提供服务支持；

6、运费承担

  我们强烈建议客户到当地经销商购买我们的产品，而当地经销也会乐意为您提供一流的售后服务。

为了保证经销商的利益，我们会对不在当地经销商购买的产品提供直接的售后服务，但是寄回产品给我们的运费需由客户承担。

Warranty Service

1. Free Repair/Replacement within 15 Days after Receipt

Within 15days after receipt and under normal use, any quality problem with your SUNWAYMAN flashlight, you can either send the light to repair or a new one of the same type with same specifications will be replaced; if the same model has been discontinued or not able to be replaced timely due to other reasons, another model with same or better performance will be replaced instead;

2. 24 Months' Free Repair

Within 24months after receipt and under normal use, any quality problem with your SUNWAYMAN flashlight, you can send it to repair for free;

3. Lifetime Limited Maintenance

SUNWAYMAN provides you with lifetime limited maintenance for your flashlight, after the 24 months' free repair period, any problems with your flashlight, SUNWAYMAN can repair and maintain it, repairing fee will be charged on an actual material cost basis, no labor cost charged;

4. Internet Warranty Card Registration

SUNWAYMAN recommends that you go to www.sunwayman.com Customer Service column to register the one and only serial number on your flashlight, after successful registration, you will be able to get another 6 months' free repair period at no cost, and your flashlight will enjoy in all 30 months' free warranty service;

5. Contact Your Dealer First

You will provide your SUNWAYMAN Warranty Card, purchasing invoice or any documents from on-line dealers and contact your dealers directly for warranty service, and SUNWAYMAN will provide dealers with service support;

6. Shipping Cost

 We strongly recommend consumers to go to their local official dealers to purchase our products, and our local dealers will be happy to provide you with an excellent after-sale service.

In order to protect the rights of our dealers, we will be directly responsible for after-sale service if products not purchased through our local dealers, but the return shipping cost is to be borne by the consumers themselves.